1. Copy the '3353efi' folder onto a USB flash drive.
2. Access the BIOS settings, disable 'Trusted Computing,' save the changes, and restart your computer.
3. Launch the EFI shell.
4. Navigate to the '3353efi' folder.
5. Enter the command 'update.nsh.'
6. You will see a message indicating that the Infineon SLB9665 firmware is being updated.
7. Once the update is successful, enter the command 'reset -s' to shut down the computer.
8. Re-enter the BIOS settings, enable 'Trusted Computing,' save the changes, and restart your computer.
9. Verify the TPM status in Windows 11.